Index

action id, pixels, 81 action id, strips, 64 action id, system, 21 addresses, base, system, 26 assemble header, 32 assemble header, 50 assemble trigdat, 41 base addresses, system, 26 boot process, 8 buffer, data, 50 buffer, message, 47 burst, signals, 8 burst det init, pixels, 91 burst det init, strips, 75 burst det init, 54 burst init, 41 burst status, 41 calibrate, 41 calibration, 9 calib init, pixels, 91 calib init, strips, 75 calib init, 54 check mess, 41 clear indata buf, pixels, 91 clear indata buf, strips, 75 code development, UCI Sun, 93 code, DSP, 15 code, strips, 60 code, system, 17 code, user, 47 data buffer, pixels, 79 data buffer, strips, 60 data buffer, 50 data collecting, user code, 55 data format, general, 14 data format, pixels, 83 data format, strips, 67 data reporting, user code, 56 data transfer, 46 data transfer, 9 data ready, pixels, 91 data ready, strips, 75 data ready, 55 data summary, 41 data transfer, 41 defaults, pixels, 82 defaults, strips, 66 defaults, system, 26 det init, pixels, 91 det init, strips, 75 det init, 54 disable link, strips, 75 disable readout, 41 dispatch specific, pixels, 91 dispatch specific, strips, 75 dispatch specific, 48 dispatch universal, 41 dis enable link, strips, 75 DSP code, development on UCI Sun, 93 DSP code, 15 DSP states, 8 echo reply, 41 enable link, strips, 75 enable link, 75 enable readout, 41 end of burst signal, 8 EOB TRANSFER, 9 error codes, pixels, 81 error codes, strips, 65 error codes, system, 25 error codes, user, 58 error report, 58 execute action, 42 execute control block, strips, 75 exec calib, pixels, 91 exec calib, strips, 75 exec calib, 55 exe control, strips, 75

97 exe control packed, strips, 75 exe trig calib, 32 exe trig calib, 55 export message, 32 export message, 50 fatal error, 58 finish readout, 42 flags, system, 22 flags, trigger flag, 9 flags, user code, 57 flags, verbose, 57 flags, verbose, 7 functions, list, user, 58 functions, pixels, alph. list, 91 functions, pixels, 88 functions, service, alph. list, 32 functions, strips, alph. list, 75 functions, strips, list, 71 functions, system service, 30 functions, system, alph. list, 41 functions, system, 34 generic message, 47 get abort flag, 32 get abort flag, 57 get action id, 42 get bit, 32 get code ver, 42 get com code ver, 42 get data blocks, pixels, 91 get data summary, pixels, 91 get data summary, strips, 76 get data summary, 56 get det status, strips, 76 get dsp status, 42 get flag, 22 get flag, 32 get flag, 57 get gray, 42 get LL status, strips, 76 get trig records, 32 get trig records, 56 get user code ver, pixels, 91 get user code ver, strips, 76 get user code ver, 54 get verbose flag, 32 get verbose flag, 57 handle message, 43 header, 48 import message, 43 initialize, 43 init a fifo, 43 init mem, 43 init regs, 43 init timer, 43 init t fifo, 43 init user var, pixels, 91 init user var, strips, 76 init user var, 54 init, 43 int a max, 32 int max, 32 LED’s, 58 load control block, strips, 76 load ctr block, strips, 76 load data block, pixels, 91 load data block, strips, 77 load data block, 55 load data, 43 load exe ctr blk, strips, 76 load graycode pattern, 44 load gray, 43 load mask, pixels, 92 load masks, pixels, 92 low level card, pixels, 86 low level card, ports, 52 low level card, strips, 70 low level card, 52 memory, data buffer, 50 memory, 47 message buffer, 47 message header, 48 message pointer, 47 message, generic, 47 messages, pixels, 80 messages, strips, 62 messages, strips, 63 messages, strips, 63 messages, system, 18 messages, user, 48 messages, 7 message status, 44 pixels, action id’s, 81 pixels, data buffer, 79 pixels, data format, 83 pixels, defaults, 82 pixels, error codes, 81 pixels, functions, alph. list, 91 pixels, functions, 88 pixels, low level card, 86 pixels, messages, 80 pixels, ports, 86 pixels, readout, 92 pixels, response codes, 81 pixels, user code, 79 PLL, 86 pointer, message, 47 pointers, global, 27 ports, low level card, 52 ports, pixels, 86 ports, strips, 70 ports, system, 28 readbit LL port, 32 readbit LL port, 54 readbit port, 44 readout, pixels, 92 readout eob, 44 readout rt, 44 readout, 44 read byte, strips, 77 read det, pixels, 92 read det, strips, 77 read det32, pixels, 92 read det52, pixels, 92 read LL port, 32 read LL port, 44 read LL port, 54 read packets, strips, 77 read port, 44 read trigger, 44 report data, pixels, 92 report data, strips, 77 report data, 56 report error, 32 report error, 58 reset burst sig, 44 reset io fifo, strips, 77 reset pac, pixels, 92 reset timer, 44 response codes, pixels, 81 response codes, strips, 65 response codes, system, 25 response codes, user, 58 RT TRANSFER, 9 run modes, 9 select align delay, 44 select column, pixels, 92 select readout mode, pixels, 92 select run mode, 45 select time param, 45 select trigger mode, 45 send response, 33 send response, 49 service functions, alph. list, 32 service functions, 30 set align delay, 45 set bit, 33 set burst sig, 45 set counter, strips, 77 set counter val, strips, 77 set dac, 45 set defaults, pixels, 92 set defaults, strips, 77 set defaults, 54 set flag, 22 set flag, 33 set flag, 45 set flag, 57 set led, 33 set led, 58 set LL dac, strips, 77 set LL voltage, strips, 77 set readout mode, pixels, 92 set strobe, strips, 78 set strobe delay, strips, 78 set sys defaults, 33 set sys defaults, 54 set trigger mode, 45 set voltage, 46 SLL, 70 start of burst signal, 8 store gray, 46 strips, action id, 64 strips, data format, 67 strips, defaults, 66 strips, dis/enable link, 75 strips, error codes, 65 strips, functions, alph. list, 75 strips, functions, list, 71 strips, low level card, 70 strips, messages, 62 strips, messages, 63 strips, messages, 63 strips, ports, 70 strips, response codes, 65 structure, generic, 47 system code, 17 system flags, 22 system functions, alph. list, 41 system functions, 34 system messages, 18 system ports, 28 system, action id’s, 21 system, base addresses, 26 system, defaults, 26 system, global variables, 27 system, pointers, 27 system, service functions, 30 test message, 46 transfer data, 46 trigdat ready, 46 trigger flag, 9 t clock, 33 user code, data collecting, 55 user code, data reporting, 56 user code, dispatcher, 48 user code, error codes, 58 user code, flags, 57 user code, pixels, 79 user code, ports, 52 user code, response codes, 58 user code, setup and initializations, 54 user code, strips, 60 user code, 47 user functions, list, 58 user functions, pixels, 88 user functions, strips, 71 user messages, 48 variables, global, 27 verbose flag, 57 verbose flag, 7 wait cycle, 33 wait, 33 writebit LL port, 33 writebit LL port, 53 writebit port, 46 write LL port, 33 write LL port, 53 write port, 46