6.55 x 8.4mm

cal3
cal2
cal1
cal0

IS_PR

IP_PR

D_ISH
detgnd

GNDA
vthp
vthn

GVDD (test)

DGND (test)

VCCring-a
ring-a

VCC

RESETB

DOUT0B

TKIN0

TKIN0B

DOUT0

TKOUT0

DIN0B

DIN0

TKOUT0B

DOUT1

DOUT1B

TKIN1

TKIN1B

DIN1

DIN1B

TKOUT1

TKOUT1B

ID<4>

ID<3>

ID<2>

ID<1>

ID<0>

COM0

COM0B

CLK0

CLK0B

SELECT (CLK0/1)

COM1B

COM1

CLK1B

CLK1

MASTER

LEDLEDB

VSSVSSVDDVDDVSSVDD

ABCD II

VccAgnd
ground
cleanbe changed and determined from experience

agnd, ringa, and detgnd connections may need to

LED BONDS ARE ONLY MADE AT MASTER SITES

BASIC BONDING DETAIL FOR ABCD2

BASIC BONDING DETAIL FOR ABCD

DIFFERENT AT EACH SITE _ REFER TO SCHEMATIC

+vdd

GNDGNDGNDNOTE THAT MASTER AND ID BONDS ARE