test2
test0

VT2VT1VCCA-GND
ring-a

AGND goes to strip bias

N.B. HT may not be needed

OF SUBSTRATE

CORNER OF BOTTOM SIDE

AND GROUND AT TOP LH

BONDING OF DETECTOR HT

FANOUT

GNDHT