are not mirrored - detector is fed from RHS only.

only right half shown, chip conns are same on LHS but detector connectons
best configuration so far but difference of ring-a to agnd or clean gnd is marginal
chip6
chip5
chip4

Putting 1.5k in R increases noise and pulls down efficiency below 100%

R3 and R4 are 10 ohms only because no 0 ohm links were available

BUT shorting out the 10 ohms in R3 makes little difference
tony smith feb 99
dgnd

Aluminium foil under chips giving backplane connection
star
point

ACLEAN GROUND - intended for cafe

10nf
agnd
ring-a
ring-aForward hybrid ground and bias configuration

lines except on hybrid.

note - no common between these

Power returns
no connection to any ground on support card
this comes straight in from the supply

Note - no components on support card

Bias

STRIP BIAS

DETECTOR BIAS

DGND

AGND

AGND

DGND

R3 10R

R4 10k

R2 10R

R1 10k